

**RDB CPLD programming**


**Install Altera programmer**:




Double click ‘QuartusProgrammerSetup’




Click Next




Select ‘I accept the agreement” and click Next.



Click next




Click next





Click Finish


**Program CPLD**:

Power down board and connect programmer. Power up board and launch ‘Quartus II 32-bit Programmer’.












Click on ‘Hardware Setup’




Double click USB-Blaster then close



Click ‘Add File’



Browse to file, select it and click open.



File shows in the window. Click check boxes ‘Program/configure’ and ‘verify’ then click ‘Start’. This programs the CPLD and verifies it.

Check the ‘Messages’ window that the verify was successful.

Power down board and unplug the programmer.